**ABHA INTERNATIONAL AIRPORT (AHB) – W24 CAPACITY DECLARATION**

**Runway**

Open H24

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  | | --- | --- | --- | --- | | **R60 Slot Capacity Limit** | | | | | **Hours (UTC)** | Arrival | Departure | **Total** | | 0000-2300 | 10 | 10 | **20** | | |  |  |  |  | | --- | --- | --- | --- | | **R15 Slot Capacity Limit** | | | | | **Hours (UTC)** | Arrival | Departure | **Total** | | 0000-2300 | 4 | 4 | **8** | |

**Terminal**

Domestic International

|  |  |  |
| --- | --- | --- |
| **T60/15 Terminal Capacity Limit** | | |
| **Hours (UTC)** | Arrival | Departure |
| 0000-2300 | 800 | 800 |
| Load Factor: 90% | | |

|  |  |  |
| --- | --- | --- |
| **T60/15 Terminal Capacity Limit** | | |
| **Hours (UTC)** | Arrival | Departure |
| 0000-2300 | 300 | 300 |
| Load Factor: 90% | | |

**Check-in**

18 counters. International flights open 180 minutes before STD, closes 60 minutes before STD. Domestic widebody flights open 165 minutes before STD, closes 45 minutes before STD. Domestic narrowbody flights open 135 minutes before STD, closes 45 minutes before STD.

International flights 3 counters per narrowbody. Domestic flights 2 counters per widebody and 1 counter per narrowbody.

1 counter reserved for Saudia Business and 1 counter reserved for Flynas.

**Gates**

5 Gates for domestic, 2 Gates for International. Maximum of 5 Gates utilised in a rolling hour.

**Apron Parking**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  | | --- | --- | --- | --- | | **Apron 1** | | | | | **ICAO aircraft size** | Options | Options | Options | | Code C | 7 | 3 | 2 | | Code E | - | 4 | 5 | | **Total** | 7 | 7 | 7 | | |  |  | | --- | --- | | **Apron 2** | | | **ICAO aircraft size** | Options | | Code C | 6 | | Code E | - | | **Total** | 6 | |

**Miscellaneous**

ICAO Code F aircraft are not permitted to operate.

Separation of 10 minutes must be applied for every domestic departure flight. Separation of 60 minutes for every international arrival flight, Airport Administration prohibits airlines from scheduling different time slots for international flights for different days.

The terminal is undergoing an expansion, and shall be done by 20 SEP 2024, before the declaration of W24 activation date. Therefore, all the numbers and capacities mentioned, will reflect the terminal expansion once it’s done.

GABA slot requests are managed by airport directly.